% $Header: /cvsroot/latex-beamer/latex-beamer/solutions/conference-talks/conference-ornate-20min.en.tex,v 1.7 2007/01/28 20:48:23 tantau Exp $

\documentclass{beamer}

% This file is a solution template for:

% - Talk at a conference/colloquium.
% - Talk length is about 20min.
% - Style is ornate.



% Copyright 2004 by Till Tantau <tantau@users.sourceforge.net>.
%
% In principle, this file can be redistributed and/or modified under
% the terms of the GNU Public License, version 2.
%
% However, this file is supposed to be a template to be modified
% for your own needs. For this reason, if you use this file as a
% template and not specifically distribute it as part of a another
% package/program, I grant the extra permission to freely copy and
% modify this file as you see fit and even to delete this copyright
% notice. 


\mode<presentation>
{
  \usetheme{Warsaw}
  % or ...

  \setbeamercovered{transparent}
  % or whatever (possibly just delete it)
}


\usepackage[english]{babel}
% or whatever

\usepackage[latin1]{inputenc}
% or whatever

\usepackage{times}
\usepackage[T1]{fontenc}
% Or whatever. Note that the encoding and the font should match. If T1
% does not look nice, try deleting the line with the fontenc.


\title{Opening Closed Domains\\Examples: RFID, DECT, GSM}

\subtitle
{A hackers journey through technology}

\author{Harald Welte}

\institute
{gnumonks.org\\gpl-violations.org\\OpenBSC\\airprobe.org\\hmw-consulting.de}
% - Use the \inst command only if there are several affiliations.
% - Keep it simple, no one is interested in your street address.

\date[foss.in/2009] % (optional, should be abbreviation of conference name)
{FOSS.in conference, December 2009, Bangalore/India}
% - Either use conference name or its abbreviation.
% - Not really informative to the audience, more for people (including
%   yourself) who are reading the slides online

\subject{Free Software}
% This is only inserted into the PDF information catalog. Can be left
% out. 



% If you have a file called "university-logo-filename.xxx", where xxx
% is a graphic format that can be processed by latex or pdflatex,
% resp., then you can add a logo as follows:

% \pgfdeclareimage[height=0.5cm]{university-logo}{university-logo-filename}
% \logo{\pgfuseimage{university-logo}}



% Delete this, if you do not want the table of contents to pop up at
% the beginning of each subsection:
%\AtBeginSubsection[]
%{
%  \begin{frame}<beamer>{Outline}
%    \tableofcontents[currentsection,currentsubsection]
%  \end{frame}
%}


% If you wish to uncover everything in a step-wise fashion, uncomment
% the following command: 

%\beamerdefaultoverlayspecification{<+->}


\begin{document}

\begin{frame}
  \titlepage
\end{frame}

\begin{frame}{Outline}
  \tableofcontents
  % You might wish to add the option [pausesections]
\end{frame}


% Structuring a talk is a difficult task and the following structure
% may not be suitable. Here are some rules that apply for this
% solution: 

% - Exactly two or three sections (other than the summary).
% - At *most* three subsections per section.
% - Talk about 30s to 2min per frame. So there should be between about
%   15 and 30 frames, all told.

% - A conference audience is likely to know very little of what you
%   are going to talk about. So *simplify*!
% - In a 20min talk, getting the main ideas across is hard
%   enough. Leave out details, even if it means being less precise than
%   you think necessary.
% - If you omit details that are vital to the proof/implementation,
%   just say so once. Everybody will be happy with that.

\begin{frame}{About the speaker}
\begin{itemize}
	\item Using + playing with Linux since 1994
	\item Kernel / bootloader / driver / firmware development since 1999
	\item IT security specialist, focus on network protocol security
	\item Some board-level Electrical Engineering
	\item Expert on Free Software licensing (gpl-violations.org)
\end{itemize}
\end{frame}

\section{The FOSS success story}

\subsection{FOSS is successful}

\begin{frame}{FOSS is successful}
Free and Open Source Software is successful
\begin{itemize}
	\item As a general purpose Operating System
	\item In the Internet and Intranet server market, data centers
	\item Networking infrastructure (routers, switches, wifi AP)
	\item Workstation / Desktop Market
	\item Now Netbooks and MID's
\end{itemize}
Common denominator: (Inter)networked device
\end{frame}

\begin{frame}{Linux/FOSS and the Internet}
\begin{itemize}
	\item Imagine the state of the Linux kernel or other FOSS community without the internet
	\item Imagine working on a FOSS project without Internet access
	\item Imagine even using a typical Linux system without Internet access (apt-get / yum / ...)
\end{itemize}
Thus, the current state of FOSS cannot be explained without the success of the Internet as communication and distribution medium.
\end{frame}


\begin{frame}{Why FOSS?}

\begin{itemize}
	\item Education
	\begin{itemize}
		\item Learning by reading the source code 
	\end{itemize}
	\pause
	\item Security
	\begin{itemize}
		\item Review the source for backdoors, exploitable bugs, ...
	\end{itemize}
	\pause
	\item Modification
	\begin{itemize}
		\item Experiments, Rapid prototyping, test of new ideas
	\end{itemize}
	\pause
	\item Research possible for anyone
	\pause
	\item No vendor lock-in
\end{itemize}
\end{frame}

\begin{frame}{So everything is great?}
\begin{itemize}
	\item We have multiple FOSS OS kernels
	\item We have thousands of FOSS application programs
	\item But: Many areas of computing typically have no FOSS at all, e.g.
	\begin{itemize}
		\item RFID protocols
		\item DECT protocols
		\item GSM/UMTS/CDMA protocols
	\end{itemize}
	\item Why those three examples?
	\begin{itemize}
		\item communications infrastructure is vital for everyone
		\item big interest in verifiable/auditable privacy and security
	\end{itemize}
\end{itemize}
\end{frame}

\subsection{Why no FOSS in RFID, DECT and GSM}

\begin{frame}{Why do you think there no FOSS?}{In RFID DECT and GSM}
\begin{itemize}
	\item No Open specifications for the protocols?
	\pause
	\begin{itemize}
		\item WRONG: They're all publicly available to anyone
	\end{itemize}
	\pause
	\item Too close to the hardware for FOSS developers
	\pause
	\begin{itemize}
		\item WRONG: Look at FOSS softmac wifi drivers
	\end{itemize}
	\pause
	\item Hardware comes without specs
	\pause
	\begin{itemize}
		\item TRUE, but look at reverse engineerd 3D drivers
	\end{itemize}
	\pause
	\item Too complex for FOSS developers
	\pause
	\begin{itemize}
		\item WRONG, look at image processing or a TCP/IP protocol stack
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{Why there really is no FOSS?}{In RFID DECT and GSM}
\begin{itemize}
	\item RFID, DECT and GSM are hardware industry dominated areas
	\begin{itemize}
		\item If you think the software industry took 10-15 years to realize the benefits of FOSS, try to imagine how long it will take the hardware and semiconductor industry
	\end{itemize}
	\item Semiconductor industry actively keeping customers out and ensure their own turf is as big as possible
	\item Chicken-and-egg Problem
	\begin{itemize}
		\item Too little people know about the protocol
		\item Too little people are able to work on FOSS for it
		\item Too little FOSS in that area
		\item Nobody can experiment with / learn from FOSS -> Too little people know about the protocol
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{Why did I care?}
\begin{itemize}
	\item because I use cordless phones, cellphones and RFID
	\item because I know and am used to the benefits of FOSS for 15 years
	\item because I don't see why I should give up that freedom when leaving the PC world
\end{itemize}
\end{frame}

\begin{frame}{What could be done about that?}
\begin{itemize}
	\item Tackle those cases, one by one
	\item Even a single person or a small group of people can make a huge difference
	\item None of the projects that were started to change this involved more than a handful of people
	\item There are no limits other than those of your mind!
\end{itemize}
\end{frame}


\section{Case studies}

\subsection{RFID}

\begin{frame}{Why my interest in RFID?}
\begin{itemize}
	\item In November 2005, the German federal government has started to issue electronic passports with RFID interface.
	\item All other EU member states were mandated to start issuing such passports no later than January 2007
	\item Passports with RF interface raise lots of security questions
	\begin{itemize}
		\item Can you track/identify a person?
		\item Can you determine his nationality?
		\item Is the crypto used sufficient to prevent forgeries?
	\end{itemize}
	\item Thus, in 2005 I realized: FOSS for RFID protocol + ePassport application is needed
\end{itemize}
\end{frame}

\begin{frame}{RFID products}{commercially available readers}
\begin{itemize}
	\item There are many RFID readers, some even with Linux drivers
	\item All the protocol logic typically happens inside reader firmware
	\item Application programmer presented with high-level API (PC/SC)
	\item No way of doing actual practical protocol-level security research
\end{itemize}
\end{frame}

\begin{frame}{RFID products}{Semiconductors}
\begin{itemize}
	\item Inside a reader, you need to somehow implement the radio layer
	\item Typically, for mass-produced products, you use integrated circuits
	\item The early RFID ASICs were dumb transceivers with no protocol logic
	\item ASIC Documentation for NXP RC5xx {\em almost} openly avaiable as 40-bit {\em encrypted} PDF
	\item Some readers export those ASIC registers to PC software and run protocol stack in proprietary software
\end{itemize}
\end{frame}

\begin{frame}{Project librfid}
\begin{itemize}
	\item Project librfid was born
	\item The first FOSS protocol stack for RFID protocols
	\begin{itemize}
		\item ISO 14443-1,2,3,4 (specification public)
		\item ISO 15693 (specification public)
		\item Mifare Classic (vendor-specific proprietary system)
	\end{itemize}
	\item Mainly written by one person!
\end{itemize}
\end{frame}

\begin{frame}{More FOSS for RFID}{OpenPCD}
OpenPCD
\begin{itemize}
	\item Project OpenPCD developed an open hardware RFID reader
	\item FOSS firmware, cross-compiled with avr-gcc, installed with FOSS flashing tools
	\item librfid used as protocol stack either inside reader firmware or on host PC
	\item R\&D done by three people!
\end{itemize}
OpenPICC
\begin{itemize}
	\item Project OpenPICC developed an open hardware RFID simulator
	\item R\&D by three people in their spare time!
\end{itemize}
\end{frame}

\begin{frame}{More FOSS for RFID}{OpenPCD}
\begin{itemize}
	\item Various groups started RFID security research on proprietay RFID standards
	\begin{itemize}
		\item Wrong security claims by RFID industry could be revealed as part of the Mifare Classic CRYPTO-1 reverse engineering in 2006
		\item Industry was forced to introduce and use components with higher security
		\item Still, e-payment and access control sytstems all over the world rely on broken-by-design, proprietary and small-keysize Mifare Classic CRYPTO1.  They deserve to be hacked, and the responsible IT managers deserve to be fired.
		\item Watch 26C3 in four weeks: Yet another proprietary insecure system will die.
	\end{itemize}
\end{itemize}
\end{frame}

\subsection{DECT}

\begin{frame}{DECT systems}{What they are}
\begin{itemize}
	\item DECT means Digital European Cordless Telephony
	\item Is a standard used in large parts of the world for cordless telephony
	\item Standardized at the ETSI, documents available to everyone
	\item Authentication and Encryption algorithms kept secret
	\item Typically, all you can buy is a black-box appliance consisting of phone + base station
\end{itemize}
\end{frame}

\begin{frame}{DECT beyond just simple cordless phones}
\begin{itemize}
	\item DECT always supported the transmission of data, e.g. ISDN payloads
	\item At some point, people wanted to use their DECT handset with VoIP
	\item Companies started to sell PCMCIA, USB and PCI DECT adapters
	\item DECT protocol stack is running inside proprietary windows software
	\item DECT encryption implemented inside the DECT chipset silicon
\end{itemize}
\end{frame}

\begin{frame}{First FOSS for DECT}
\begin{itemize}
	\item In order to do research on DECT, Open Source is needed
	\item Group (later called deDECTed.org) formed doing reverse engineering of windows drivers
	\item Started to implement FOSS driver for the hardware and Receive-only processing of DECT protocol stack
	\item Was used by cryptographers as a toolbox to demonstrate that the DECT Security is not worth the paper it is printed on
	\begin{itemize}
		\item Problems in the protocol specification
		\item Problems in the implementations (16bit random numbers?!?)
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{More FOSS for DECT}
\begin{itemize}
	\item Patrick McHardy (netfilter/iptables maintainer) starts a Linux kernel DECT stack
	\item His experience in Linux kernel networking enables him to write a true Linux network stack for the DECT protocol
	\item git://git.kernel.org/pub/scm/linux/kernel/git/kaber/dect-2.6.git
	\item Written by one person!
\end{itemize}
\end{frame}

\subsection{GSM}

\begin{frame}{The closed GSM industry}{Handset manufacturing side}
\begin{itemize}
	\item Only very few companies build GSM/3.5G baseband chips today
	\begin{itemize}
		\item Those companies buy the operating system kernel and the protocol stack from third parties
	\end{itemize}
	\item Only very few handset makers are large enough to become a customer
	\begin{itemize}
		\item Even they only get limited access to hardware documentation
		\item Even they never really get access to the firmware source
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{The closed GSM industry}{Network manufacturing side}
\begin{itemize}
	\item Only very few companies build GSM network equipment
	\begin{itemize}
		\item Basically only Ericsson, Nokia-Siemens, Alcatel-Lucent and Huawei
		\item Exception: Small equipment manufacturers for picocell / nanocell / femtocells / measurement devices and law enforcement equipment
	\end{itemize}
	\item Only operators buy equipment from them
	\item Since the quantities are low, the prices are extremely high
	\begin{itemize}
		\item e.g. for a BTS, easily 10-40k EUR
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{The closed GSM industry}{Operator side}
\begin{itemize}
	\item Operators are mainly banks today
	\item Typical operator outsources
	\begin{itemize}
		\item Billing
		\item Network planning / deployment / servicing
	\end{itemize}
	\item Operator just knows the closed equipment as shipped by manufacturer
	\item Very few people at an operator have knowledge of the protocol beyond what's needed for operations and maintenance
\end{itemize}
\end{frame}

\begin{frame}{The closed GSM industry}{Security implications}
The security implications of the closed GSM industry are:
\begin{itemize}
	\item Almost no people who have detailed technical knowledge outside the protocol stack or GSM network equipment manufacturers
	\item No independent research on protocol-level security
	\begin{itemize}
		\item If there's security research at all, then only theoretical (like the A5/2 and A5/1 cryptanalysis)
		\item Or on application level (e.g. mobile malware)
	\end{itemize}
	\item No open source protocol implementations
	\begin{itemize}
		\item which are key for making more people learn about the protocols
		\item which enable quick prototyping/testing by modifying existing code
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{Security analysis of GSM}{How would you get started?}
If you were to start with GSM protocol level security analysis, where and
how would you start?
\begin{itemize}
	\item On the handset side?
	\begin{itemize}
		\item Difficult since GSM firmware and protocol stacks are closed and proprietary
		\item Even if you want to write your own protocol stack, the layer 1 hardware and signal processing is closed and undocumented, too
		\item Known attempts
		\begin{itemize}
			\item The TSM30 project as part of the THC GSM project
			\item mados, an alternative OS for Nokia DTC3 phones
		\end{itemize}
		\item none of those projects successful so far
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{Security analysis of GSM}{How would you get started?}
If you were to start with GSM protocol level security analysis, where and
how would you start?
\begin{itemize}
	\item On the network side?
	\begin{itemize}
		\item Difficult since equipment is not easily available and normally extremely expensive
		\item However, network is very modular and has many standardized/documented interfaces
		\item Thus, if equipment is available, much easier/faster progress
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{Security analysis of GSM}{The bootstrapping process}
\begin{itemize}
	\item Read GSM specs day and night (> 1000 PDF documents)
	\item Gradually grow knowledge about the protocols
	\item Obtain actual GSM network equipment (BTS)
	\item Try to get actual protocol traces as examples
	\item Start a complete protocol stack implementation from scratch
	\item Finally, go and play with GSM protocol security
\end{itemize}
\end{frame}

\begin{frame}{OpenBSC}{A FOSS GSM protocol stack implementation}
\begin{itemize}
	\item OpenBSC implements {\em GSM network in a box}
	\begin{itemize}
		\item BSC, MSC, HLR, AuC, ...
		\item You can use a BTS + OpenBSC and run your own network
	\end{itemize}
	\item Commercial systems with same functionality sell for >~50,000 USD
	\begin{itemize}
		\item Did you also hear the romours about 100-man-years intellectual property in a GSM stack?
	\end{itemize}
	\item Developed by three people in their spare time!
\end{itemize}
\end{frame}

\begin{frame}{OpenBTS}{A different GSM protocol stack implementation}
\begin{itemize}
	\item Open implementation of Um L1 \& L2, an all-software BTS.
	\item L1/L2 design based on an object-oriented dataflow approach.
	\item Includes L3 RR functions normally found in BSC.
	\item Uses SIP PBX for MM and CC functions, eliminating the conventional GSM network.  L3 is like an ISDN/SIP gateway.
	\item Intended for use in low-cost and rapidly-deployed communications networks, but can be used for experiments.
	\item Written by two people!
\end{itemize}
\end{frame}

\begin{frame}{airprobe}{A GSM receiver / protocol analyzer}
\begin{itemize}
	\item {\em airprobe} is a collection of Um protocol analyzer tools using the USRP software defined radio
	\item A number of different Um receiver implementations
	\begin{description}[gsm-receiver]
		\item[gssm] One of the two early Um receiver implementations (M\&M clock recovery)
		\item[gsmsp] The other early Um receiver implementation
		\item[gsm-tvoid] For a long time the Um receiver with best performance
		\item[gsm-receiver] The latest generation of Um receiver
	\end{description}
	\item Today, gsm-receiver seems to be the most popular choice
\end{itemize}
\end{frame}

\begin{frame}{What has GSM FOSS shown?}
\begin{itemize}
	\item We can now do real-world demonstration of GSM weaknesses
	\begin{itemize}
		\item Lack of mutual authentication
		\item Silent calls to turn phones into permanently transmitting beacons
		\item RRLP to inquire the GPS fix of any phone
	\end{itemize}
	\item We can make people aware of the dangers those features have
	\item Hopefully, public pressure will force the industry to change
\end{itemize}
\end{frame}

\section{Summary}

\subsection{What we've learned}

\begin{frame}{Summary}{What we've learned}
\begin{itemize}
	\item There are many areas which the benefits of FOSS have not yet reached
	\item Nonetheless, those systems are used by billions of people every day
	\item Without independent research, security flaws will never be removed
	\item Small projects with few dedicated developers can make a huge impact
\end{itemize}
\end{frame}

\subsection{Get involved!}

\begin{frame}{Get involved!}
\begin{itemize}
	\item Boldly go where no (FOSS) man has gone before
	\item Don't be deterred by people who say it's impossible
	\item What are you waiting for?
	\item Would you rather become the worlds 10,000th application security expert or the worlds 100th GSM protocol security expert?
	\item Help us to get some sense into the semiconductor industry.
\end{itemize}
\end{frame}

\subsection{Knowledge is power}

\begin{frame}{Knowledge is power}
\begin{itemize}
	\item Educate yourself
	\item Never underestimate {\em learning by doing}
	\item Educate others about 
	\begin{itemize}
		\item How every-day technology like cellphones really work
		\item What is the true security and privacy level of those systems
	\end{itemize}
\end{itemize}
\end{frame}

\begin{frame}{Where to go?}{Areas that need openness}
\begin{itemize}
	\item 3G (UMTS) protocol stack
	\item GSM telephone side GSM stack
	\item What about DAB, DMB-T
	\item DVB-S encapsulated Internet downlink
	\item TETRA being deployed in multiple European countries
	\item CDMA / CDMA2000
	\pause
	\item ... and this is just in the communications protocol sector!
\end{itemize}
\end{frame}

\end{document}
